**SCOPE**

**GENERAL DESCRIPTION AND OPERATION**

**1.1 PROJECT DESCRIPTION**

The project comprises the installation of Hydraulic services for Assisi Stage 2

The Hydraulic services installation entails the following

* Sewer drainage
* Hot ,Cold and Warm water service
* Below ground Hydrant Fire Service
* Stormwater drainage
* 12 months free warranty

**1.2 WORK CARRIED OUT**

The Hydraulic services comprise a New Sewer drainage system with connections to existing Manholes, New Hot, Cold and Warm water service, New Below ground Hydrant Fire Service and New Stormwater drainage system with connections to existing drains.

Pipework Materials

* Sewer drainage – PVC
* Hot ,Cold and Warm water service – Copper and PEX
* Below ground Fire Service – Copper and Polyethylene
* Stormwater drainage – PVC