**WORK CARRIED OUT**

**HYDRANT FIRE SERVICE >**

The Existing 100mm copper service located in the lawn area on the Eastern side of Stage 3 is connected to a new 125mm poly line. There is a 100mm sluice valve located outside the Plantroom on the South Eastern corner of Stage 3 . 125mm electrofusion welded Poly pipe PN16 with copper riser extends up into the new plantroom under stage 3. This riser is fitted with a Rollgrove adaptor. 100mm galvanised rolled grove pipe is suspended at high level connecting the new fire hydrant located on the south east balcony. These valves, fire hydrants and pipe locations are noted on as constructed drawings.