**SCOPE**

**GENERAL DESCRIPTION AND OPERATION**

**1.1 PROJECT DESCRIPTION**

The project comprises the installation of Hydraulic services for Assisi Stage 3

The Hydraulic services installation entails the following

* Sewer drainage
* Hot ,Cold and Warm water service
* Below ground Hydrant Fire Service
* Stormwater drainage
* 12 months free warranty

**1.2 WORK CARRIED OUT**

The Hydraulic services comprise a New Sewer drainage system with connections to existing Sewer Drains, New Hot, Cold and Warm water service with connections to existing Domestic Cold Water supply and Stage 2 Hot Water Plant, New Below ground Hydrant Fire Service and New Stormwater drainage system with connections to existing drains.

Pipework Materials

* Sewer drainage – PVC
* Hot ,Cold and Warm water service – Copper and PEX
* Below ground Fire Service – Copper and Polyethylene
* Stormwater drainage – PVC